#!/bin/bash

# Stop eth0 (ethernet) if it's running
started=0

if /etc/init.d/net.eth0 status | grep "started" >/dev/null ; then
	started=1
fi

if test "${started}" = "1" ; then
	/etc/init.d/net.eth0 stop
fi

# Stop eth1 (wireless) if it's running
started=0

if /etc/init.d/net.eth1 status | grep "started" >/dev/null ; then
	started=1
fi

if test "${started}" = "1" ; then
	/etc/init.d/net.eth1 stop
fi

modprobe -r eth1 2>/dev/null
