# /etc/conf.d/g15daemon: Configuration for the g15daemon

# Key to switch the client-screens. Default is the MR key,
# Set to "yes" to use L1 key instead (black round key below the LCD, above the multimedia keys).
CLIENT_SWITCH_L1="no"

# Set to "yes" to switch off the lcd backlight when stopping g15daemon.
BACKLIGHT_OFF="no"

